MERG DCC System Demonstration

This uses MERG's DCC Command Station (kit 91) connected to MERG's DCC Handset (kit 92) via the CANRJ22 connector (kit 92V). A CAB Holder (kit 673) is used to hold the Handset.

The track is divided into 7 sections and the DTC8 DCC Block Detector (kit 56) used to show track occupancy. The DTC8 is split into 4 boards, each with 2 coils and these are fed into the CBUS System

back to photo